CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.1/conf/instr/spect/uxnmr.info
Date         : Fri Mar 13 15:59:04 2015
Release      : TopSpin Acquisition Version 3.1-pl6
Installed in : /opt/topspin3.1
Host         : CZC01362SB
OS           : CentOS release 5.5 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : nmrsu (NMR Administrator (nmrsu))
Description  : Avance III 500
Location     : IISER
System       : Avance III NMR spectrometer
1H-frequency : 500.13 MHz
Order Number : 10016680
Configured in: /opt/topspin3.1/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/01948 ECL 06.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.4 REC-1  AQS RXAD600 Z102117/941 ECL 04.04
     3   0x34 0xc9   0x1        X  1.2 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x19   0x8    AE  S  2.7 SGU-1  AQS SGU/2 600 Z103081/01993 ECL 02.07 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.7 SGU-2  AQS SGU/2 600 Z103081/01996 ECL 02.07 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.7 SGU-3  AQS SGU/2 600 Z103081/01994 ECL 02.07 FPGA-Vs=AF
     7   0x27 0x19   0x8    AE  S  2.7 SGU-4  AQS SGU/2 600 Z103081/01995 ECL 02.07 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345099_0156 W1345099/0156 ECL 2:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/150 E 200-600MHZ INR: W1345099/0156 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0940 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/4901 ECL 05
- QNP-Accessory  : 1 X-input and 1 H-input
BLA_W1345093_0336 W1345093/0336 ECL 1:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0336 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1230 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/4914 ECL 05
LTRX Z109889/00134 ECL 01.02:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00134 ECL 01.02

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130320
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00134 ECL 01.02
- Lock: on L-TRX board

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty04
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AP
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003461, SN=00901 from 20100514
    Module  2 : XBB19F 2HS
                 PN=Z003505, SN=00906 from 20100429
    Module  3 : XBB19F 2HS
                 PN=Z003505, SN=00905 from 20100429
    Module  4 : 2H
                 PN=Z003472, SN=00844 from 20100505


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0336 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253)
SGU3 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0336 at TCP/IP 149.236.99.252)
SGU4 NORM output -> input 3 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0336 at TCP/IP 149.236.99.252)
SGU4 AUX  output -> input 4 of transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253) amplifier X-500W uses blanking 1
transmitter 1 (BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253) amplifier 2H-150W needs no blanking
transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0336 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 3
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 500 Z109889/00134 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253 amplifier X-500W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253 amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
BLAXH2H500/100/150 E 200-600MHZ W1345099/0156 at TCP/IP 149.236.99.253 amplifier 2H-150W can be routed to switchbox output 5 (unknown)

