Parameters for C:\MassLynx\DEFAULT.PRO\ACQUDB\+296.EXP
Created by Masslynx v4.1
 
Lock Spray Configuration:
Reference Scan Frequency(sec)		10.000
Reference Cone Voltage(V)		45.000
 
Temperature Correction:
Temperature Correction			Disabled
 
Instrument Configuration:
Trigger Threshold				650
Signal Threshold				35
T0Constant				-50
Lteff				1400.0
Veff				5520.86
Centroid Threshold				1
Min Points in Peak				2
Np Multiplier				0.700
Resolution				9000
EDC Delay Coefficient			1.4300
EDC Delay Offset			-1.0000
Maldi Laser Firing Rate			1.0
Maldi Plate Speed			1.0
Maldi Laser Energy			250.0
Maldi Pattern Filename			c:\Masslynx\Spiral_96.ptn
Maldi Lock Mass Pattern File			c:\Masslynx\Spiral_96.ptn
Tof Emulation Transfer Pulse Height (V)	0.1
 
Experimental Instrument Parameters
Instrument Parameter Filename		C:\MassLynx\Default.pro\Acqudb\20200905.ipr
Polarity				ES+
Analyser				V Mode
Capillary (kV)	1.5
Sampling Cone	5.0
Extraction Cone	4.0
Source Temperature (°C)	100
Desolvation Temperature (°C)	400
Cone Gas Flow (L/Hr)	50.0
Desolvation Gas Flow (L/Hr)	700.0
LM Resolution	4.7
HM Resolution	15.0
Aperture 1	0.0
Pre-filter	2.0
Ion Energy	1.0
Trap Collision Energy	6.0
Transfer Collision Energy	4.0
Trap Gas Flow (mL/min)	1.50
Source Gas Flow (mL/min)	0.00
IMS Gas Flow (mL/min)	24.00
Detector	2000
Pusher Interval (µS)	64
Pusher Width	4
Acceleration1	70.0
Acceleration2	200.0
Aperture2	70.0
Transport1	70.0
Transport2	70.0
Steering	0.0
Tube Lens	75
Pusher	915.0
Pusher Offset	-2.70
Puller	645.0
Photo Multiplier	650
Collector	60
Collector Pulse	10.0
Stopper	10
Stopper Pulse	20.0
Entrance	75
Static Offset	120
Puller Offset	0.00
TOF (kV)	9.10
Reflectron (kV)	2.16
Pusher Interval (µS)	64
Pusher Width	4
Trap DC Entrance	5.0
Trap DC Bias	4.0
Trap DC Exit	5.0
IMS DC Entrance	-20.0
IMS DC Exit	20.0
Transfer DC Entrance	5.0
Transfer DC Exit	15.0
Source Manual Control	OFF
Source Wave Velocity (m/s)	300
Source Wave Height (V)	0.2
Trap Manual Control	OFF
Trap Wave Velocity (m/s)	300
Trap Wave Height (V)	0.5
IMS Manual Control	OFF
IMS Wave Velocity (m/s)	300
IMS Wave Height (V)	0.5
Transfer Manual Control	OFF
Transfer Wave Velocity (m/s)	248
Transfer Wave Height (V)	0.2
Trapping Mode/Location	Trap
Trap Manual Release Enabled	FALSE
Trap Release Time (µs)	100
Trap Trap Height (V)	10.0
Trap Extract Height (V)	5.0
IMS Manual Release Enabled	FALSE
IMS Release Time (µs)	100
IMS Trap Height (V)	10.0
IMS Extract Height (V)	5.0
EDC Enabled	FALSE
EDC Mode	EDC
EDC Mass	556.0
HDC Table	
Transfer Trap Height (V)	4.0
Transfer Extract Height (V)	15.0
Variable Wave Height Enabled	FALSE
Wave Height Ramp Type	Linear
Wave Height Start (V)	8.0
Wave Height End (V)	20.0
Wave Height Using Full IMS	TRUE
Wave Height Ramp (%)	100.0
Wave Height Look Up Table	
Variable Wave Velocity Enabled	FALSE
Wave Velocity Ramp Type	Linear
Wave Velocity Start (m/s)	300.0
Wave Velocity End (m/s)	600.0
Wave Velocity Using Full IMS	TRUE
Wave Velocity Ramp (%)	10.0
Wave Velocity Look Up Table	
IMS Bias Look Up Table Enabled	FALSE
IMS Bias Look Up Table	
Multiplier	650
Collector	60
CollectorPulse	10.0
StopperBias	10
StopperPulse	20.0
Entrance	75
CollisionCellStaticOffset	120
Offset2	0.00
TOF	9.10
Reflectron	2.16
Vacuum Lock	1.15e-3
Backing	2.49e0
Source	2.68e2
Quadrupole	OFF
Trap	6.40e-3
IMS	2.98e-4
TOF	5.72e-7
SourceRFOffset	350
SourceRFGain	0
SourceRFLimit	450
IMSRFOffset	350
IMSRFGain	0
IMSRFLimit	380
TrapRFOffset	350
TrapRFGain	0
TrapRFLimit	380
TransferRFOffset	350
TransferRFGain	0
TransferRFLimit	380
MS Profile Type	Profile
MSProfileMass1	100
MSProfileDwellTime1	20
MSProfileRampTime1	20
MSProfileMass2	800
MSProfileDwellTime2	30
MSProfileRampTime2	30
MSProfileMass3	1200
 
 
Function Parameters - Function 1 - TOF MSMS FUNCTION
Scan Time (sec)				0.500
Interscan Time (sec)			0.020
Set Mass				296.0
Start Mass				50.0
MSMS End Mass				1000.0
Start Time (mins)			0.00
End Time (mins)				10.00
Data Format				Continuum
Use Tune Page Cone Voltage		NO
Cone Voltage (V)			20.0
Use Tune Page Collision Energy		NO
Collision Energy (eV)			6.0
Use Tune Page Collision Energy2		YES
Sensitivity				Normal
Dynamic Range				Normal
Save Collapsed Retention Time Data	No
Use Rule File Filtering			No
Calibration				Dynamic 2
 
Function Parameters - Function 2 - TOF MSMS FUNCTION
Scan Time (sec)				0.500
Interscan Time (sec)			0.020
Set Mass				296.0
Start Mass				50.0
MSMS End Mass				1000.0
Start Time (mins)			0.00
End Time (mins)				10.00
Data Format				Continuum
Use Tune Page Cone Voltage		NO
Cone Voltage (V)			20.0
Use Tune Page Collision Energy		NO
Collision Energy (eV)			15.0
Use Tune Page Collision Energy2		YES
Sensitivity				Normal
Dynamic Range				Normal
Save Collapsed Retention Time Data	No
Use Rule File Filtering			No
Calibration				Dynamic 2
 
Function Parameters - Function 3 - TOF MS FUNCTION
Scan Time (sec)				0.500
Interscan Time (sec)			0.020
Start Mass				50.0
End Mass				1000.0
Start Time (mins)			0.00
End Time (mins)				10.00
Data Format				Continuum
Use Tune Page Cone Voltage		NO
Cone Voltage (V)			20.0
Use Tune Page Collision Energy		NO
Collision Energy (eV)			6.0
Use Tune Page Collision Energy2		YES
Sensitivity				Normal
Dynamic Range				Normal
Save Collapsed Retention Time Data	No
Use Rule File Filtering			No
Calibration				Dynamic 2
 
Function Parameters - Function 4 - REFERENCE
Scan Time (sec)				0.50
Interval				10
Reference Cone Voltage			45.0
Collision Energy (eV)			6.0
EDC Mass				556.2771
Calibration				Dynamic 2
