{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["bodipy_test_set.xls"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"bodipy_test_set.xls","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["SMILES","Chemical shift","UNIT {Chemical shift}","Solvent","Frequency","UNIT {Frequency}"]
["CCCC1=C(C)N2C(C=C3C(C)=C(CCC)C(C)=[N+]3[B-]2(F)F)=C1C","0.896","ppm","CDCl3","= 160.0","MHz"]
["CCCCCC1=C(C)N2C(C=C3C(C)=C(CCCCC)C(C)=[N+]3[B-]2(F)F)=C1C","0.892","ppm","CDCl3","= 160.0","MHz"]
["CCCCCCC1=C(C)N2C(C=C3C(C)=C(CCCCCC)C(C)=[N+]3[B-]2(F)F)=C1C","0.896","ppm","CDCl3","= 160.0","MHz"]
["CCCCC1=C(C)N2C(C=C3C(C)=C(CCCC)C(C)=[N+]3[B-]2(F)F)=C1C","0.8929","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(CC2=CC=CC=C2)C(C)=C2C=C3C(C)=C(CC4=CC=CC=C4)C(C)=[N+]3[B-](F)(F)N12","0.9188","ppm","CDCl3","= 160.0","MHz"]
["COC(=O)CCCCC1=C2C(C)=CC(C)=[N+]2[B-](F)(F)N2C(C)=CC(C)=C12","0.5568","ppm","CDCl3","= 160.0","MHz"]
["CC1=CC(C)=C2C=C3C(C)=CC(C)=[N+]3[B-](F)(F)N12","0.8764","ppm","CDCl3","= 160.0","MHz"]
["F[B-]1(F)N2C=CC=C2C(NCC#C)=C2C=CC=[N+]12","0.1724","ppm","CDCl3","= 160.0","MHz"]
["COC(=O)CCCC1=C2C(C)=CC(C)=[N+]2[B-](F)(F)N2C=CC(C)=C12","0.5481","ppm","CDCl3","= 160.0","MHz"]
["F[B-]1(F)N2C(N=C3C(=C(Br)C(C4=CC=CC=C4)=[N+]13)C1=CC=CC=C1)=C(C(Br)=C2C1=CC=CC=C1)C1=CC=CC=C1","0.1557","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(I)C(C)=C2C=C3C(C)=C(I)C(C)=[N+]3[B-](F)(F)N12","0.6309","ppm","CDCl3","= 160.0","MHz"]
["F[B-]1(F)N2C(=CC3=C2CCCC3)C=C2C=C3CCCCC3=[N+]12","0.7094","ppm","CDCl3","= 160.0","MHz"]
["OC(=O)CCC1=CC=C2C=C3C=CC(C4=CC=CS4)=[N+]3[B-](F)(F)N12","1.3608","ppm","CDCl3","= 160.0","MHz"]
["CC1=CC(C)=[N+]2C1=CC1=CC=C(CCC(O)=O)N1[B-]2(F)F","0.9132","ppm","CDCl3","= 160.0","MHz"]
["CC1=CC(C)=C2N1[B-](F)(F)[N+]1=C(C)C=C(C)C1=C2CCCC(=O)OCC1=CCC2CC1C2(C)C","0.5517","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(C)=C2C=C3C(C)=C(C)C(CC4=C(C)C(C)=C5C=C6C(C)=C(C)C(C)=[N+]6[B-](F)(F)N45)=[N+]3[B-](F)(F)N12","0.9613","ppm","CDCl3","= 160.0","MHz"]
["CCC1=C(CC2=[N+]3C(=CC4=C(C)C(C)=C(C)N4[B-]3(F)F)C(C)=C2CC)N2C(C=C3C(C)=C(C)C(C)=[N+]3[B-]2(F)F)=C1C","0.9924","ppm","CDCl3","= 160.0","MHz"]
["CC1=CC(C)=C2C=C3C(C)=C(CC4=C(C)N5C(C=C6C(C)=CC(C)=[N+]6[B-]5(F)F)=C4C)C(C)=[N+]3[B-](F)(F)N12","0.8635","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(C)=C2C=C3C(C)=C(CC4=C(C)C(C)=C5C=C6C(C)=C(C)C(C)=[N+]6[B-](F)(F)N45)C(C)=[N+]3[B-](F)(F)N12","0.8665","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(C)=C2C=C3C(C)=C(C(C4=C(C)N5C(C=C6C(C)=C(C)C(C)=[N+]6[B-]5(F)F)=C4C)C4=CC=CC=C4)C(C)=[N+]3[B-](F)(F)N12","0.8872","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(C)=C2C=C3C(C)=C(C(C4=C(C)N5C(C=C6C(C)=C(C)C(C)=[N+]6[B-]5(F)F)=C4C)C(F)(F)F)C(C)=[N+]3[B-](F)(F)N12","0.8225","ppm","CDCl3","= 160.0","MHz"]
["CCC1=C(C)N2C(C=C3C(C)=C(CC4=C(C)N5C(C=C6C(C)=C(CC)C(C)=[N+]6[B-]5(F)F)=C4C)C(C)=[N+]3[B-]2(F)F)=C1C","0.8707","ppm","CDCl3","= 160.0","MHz"]
["COC1=CC=C(C=C1)C(C1=C(C)N2C(C=C3C(C)=C(C)C(C)=[N+]3[B-]2(F)F)=C1C)C1=C(C)C2=CC3=C(C)C(C)=C(C)N3[B-](F)(F)[N+]2=C1C","0.8949","ppm","CDCl3","= 160.0","MHz"]
["CN(C)C1=CC=C(\\C=C\\C2=CC(C)=C3N2[B-](F)(F)[N+]2=C(\\C=C\\C4=CC=C(C=C4)N(C)C)C=C(C)C2=C3C2=CC=CC=C2)C=C1","1.302","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(Br)C(C)=C2C=C3C(C)=C(Br)C(C)=[N+]3[B-](F)(F)N12","0.5515","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(Br)=C2C=C3C(C)=C(C)C(C)=[N+]3[B-](F)(F)N12","0.7475","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(Br)C(C)=C2C=C3C(C)=C(C)C(C)=[N+]3[B-](F)(F)N12","0.6999","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(Br)=C2C=C3C(Br)=C(C)C(C)=[N+]3[B-](F)(F)N12","0.6692","ppm","CDCl3","= 160.0","MHz"]
["CC1=C(C)C(C)=C2C=C3C(CC4=C(C)C(C)=[N+]5C4=CC4=C(C)C(C)=C(C)N4[B-]5(F)F)=C(C)C(C)=[N+]3[B-](F)(F)N12","0.8345","ppm","CDCl3","= 160.0","MHz"]