CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2/conf/instr/spect/uxnmr.info
Date         : Wed Jun 23 13:09:03 2021
Release      : TOPSPIN Version 3.2-pl7
Installed in : /opt/topspin3.2
Host         : a5nmr.chem.vt.edu
OS           : CentOS Linux release 7.8.2003 (Core)
CPU          : Intel(R) Xeon(R) CPU E3-1230 v5 @ 3.40GHz (8 cores at 800 MHz with Hyperthreading)
User         : nmr
Description  : Avance-AV 500
Location     : 
System       : Avance-AV NMR spectrometer
1H-frequency : 500.16 MHz
Order Number : 
Configured in: /opt/topspin3.2/conf/instr/spect

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 3 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 4 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU-E Z102520/00413 ECL 02.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619

Gcu: GCU3

AQS: connected to spect:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x3    AW  R  2.0 REC-1  AQS RXAD1000 Z102118/92 ECL 02.00
     3   0x34 0xc1   0x1        X  1.0 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x28   0x4    BH  S  6.0 SGU-1  AQS SGU1000 Z003330/01057 ECL 6.0
     5   0x25 0x28   0x4    BH  S  6.0 SGU-2  AQS SGU1000 Z003330/01066 ECL 6.0
     6   0x26 0x28   0x2    AL  S  2.5 SGU-3  AQS SGU1000 Z003330/00357 ECL 2.5
     7   0x27 0x28   0x2    AL  S  2.1 SGU-4  AQS SGU1000 Z003330/00052 ECL 2.1
     9   0x3c  0x4     0        Y  0.0 ROUT-1 Avance Router 3/5
    21   0x21  0xa     0        P  2.0 PSD-1  Power Supply Distribution Board
    23   0x20 0xc6     0        B  1.1 AQS/2  AQS/2 chassis
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 Avance-Router

Amplifier Control Board:  connected to spect:/dev/tty20


Amplifiers (ACB configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        X      500    Y  (I=ff) BLAX 500 RS W1345043/45/19970311
   2      2         1       1H      100    Y  (V=bf) BLARH 100 W1301845/381/19990407
   3      2         2       1H        1.0  Y  (-""-) BLARH 100 W1301845/381/19990407
   4      2         3       1H       10    Y  (-""-) BLARH 100 W1301845/381/19990407
   6      3         1       2H       20    N         BSMS 2HTX -/-/-



BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20180919
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: connected to router output 6
- Lock: installed

Bruker Automatic Changer: device connected to spect:/dev/tty09
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Prodigy Control Unit: PCU - LNP PRODIGY UNIT Z127349/373
- TCP/IP address   = 149.236.99.90

Eurotherm VTU: device connected to spect:/dev/tty06

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to spect:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.0%/0.1deg, reflection meter)
                 PN=Z103204, SN=00695 from 20150724
    Module  2 : XBB19F 2HS
                 PN=Z003505, SN=01053 from 20110708
    Module  3 : 2H
                 PN=Z003472, SN=00967 from 20110608


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



