CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.4/conf/instr/spect/uxnmr.info
Date         : Wed Mar 16 15:40:14 2022
Release      : TopSpin 3.6.4
Installed in : /opt/topspin3.6.4
Host         : a6nmr.chem.vt.edu
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E3-1230 v6 @ 3.50GHz (8 cores at 2737 MHz with Hyperthreading)
User         : nmr
System       : Avance III 600 NMR spectrometer
1H-frequency : 600.02 MHz
Description  : Avance III 600
Bruker Order : BH073107
Configured in: a6nmr.chem.vt.edu:/opt/topspin3.6.4/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: with digital preemphasis
- Gctrl2: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU1: AQS DRU-E Z102520/00794 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x62   0x3    AW  R  4.0 REC-1  AQS RXAD-BB Z102119/88 ECL 04.00
     3   0x34 0xc0   0x1        X  2.0 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.0 SGU-1  AQS SGU/2 600 Z103081/00524 ECL 02.00 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.0 SGU-2  AQS SGU/2 600 Z103081/00423 ECL 02.00 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.0 SGU-3  AQS SGU/2 600 Z103081/00556 ECL 02.00 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  2.1 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345095_0073 W1345095/0073 ECL 0:
- TCP/IP address = 149.236.99.95
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ: W1345095/0073 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0383 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0403 ECL 2
BLA_W1345088_0038 W1345088/0038 ECL 0:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAH1000 E 200-600MHZ: W1345088/0038 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0355 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0462 ECL 2
BLA_W1345093_0091 W1345093/0091 ECL 0:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ: W1345093/0091 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0350 ECL 0
- Controller     = BLA CONTROL BOARD 6 1V V-USB: W1522041/0189 ECL 1

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGAU_W1522066_0170
- TCP/IP address   = 149.236.99.97
- Firmware version = 20141128
- Web version      = 2.1
- Current limits   = 0.0/X, 0.0/Y, 0.0/Z (in A)
BGA2: BGA_W1213891_0044
- TCP/IP address   = 149.236.99.92
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = 0.0/X, 0.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210921
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: available
- Lock: installed

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.90:/dev/tty01
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

MAS2 control unit: connected to 149.236.99.90:/dev/tty04
- Boot Software        : 20031216
- Application Software : 20140611
- Insert Time          : 10 s
- Eject Time           : 10 s
- Spin Lock Tolerance  : 5 Hz

Eurotherm VTU: device connected to 149.236.99.90:/dev/tty05

Prodigy Control Unit: PCU - LNP PRODIGY UNIT Z127349/747
- TCP/IP address   = 149.236.99.98

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 1H19F (virtual 50 Ohm reference: 100.6%/0.0deg, reflection meter)
                PN=Z103205, SN=01187 from 20191004
    Module  2 : XBB19F 2HS
                PN=Z003506, SN=00592 from 20070628
    Module  3 : 2H
                PN=Z003473, SN=00531 from 20070702
    Module  4 : 13C/79Br
                PN=Z003524, SN=01398 from 20210201
    Module  5 : 15N
                PN=Z003530, SN=01254 from 20201126
    Module  6 : HPHP 19F/1H
                PN=Z003546, SN=00058 from 20080617
    Module  7 : HPHP XBB31P
                PN=Z003549, SN=00274 from 20070627
    Module  8 : HPHP XBB31P
                PN=Z003549, SN=00273 from 20070627



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected via DPP to GREAT MASTER UNIT E W1522066/0170
GCtrl2: connected to GREAT 1-10 Gradient Amplifier Unit W1213891/0044

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAX1000 E 6-405MHZ W1345095/0073 at TCP/IP 149.236.99.95)
SGU1 AUX  output -> input 1 of transmitter 4 (BSMS 2HTX)
SGU2 NORM output -> input 1 of transmitter 2 (BLAH1000 E 200-600MHZ W1345088/0038 at TCP/IP 149.236.99.94)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 3 (BLAX500 E 6-365MHZ W1345093/0091 at TCP/IP 149.236.99.93)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX1000 E 6-405MHZ W1345095/0073 at TCP/IP 149.236.99.95)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX1000 E 6-405MHZ W1345095/0073 at TCP/IP 149.236.99.95:
- amplifier X-1000W uses blanking 1
- amplifier X-300W uses blanking 1

transmitter 2 = BLAH1000 E 200-600MHZ W1345088/0038 at TCP/IP 149.236.99.94:
- amplifier 1H-1000W uses blanking 2
- amplifier 1H-100W uses blanking 2

transmitter 3 = BLAX500 E 6-365MHZ W1345093/0091 at TCP/IP 149.236.99.93:
- amplifier X-500W uses blanking 3

transmitter 4 = BSMS 2HTX:
- amplifier 2H-20W needs no blanking


