$CM_FORMAT JEOL/MP
$CM_VERSION 3
$CM_DATE 2021-11-22
$CM_TIME 09:07:48
$CM_OPERATOR JEOL
$CM_INSTRUMENT JSM-IT200
$CM_IMAGE_SIZE 2560 1920
$CM_COLOR_MODE 1
$CM_MAG 75
$CM_STAGE_POSITION -6.003 6.469 13.100 0.000 0.000 0.000
$CM_CONTRAST 1376
$CM_BRIGHTNESS 1844
$CM_ACCEL_VOLT 5.0
$CM_COMMENT 
$CM_LABEL 
$CM_FIELD_OF_VIEW 1.707mm 1.280mm
$CM_SEGMENT_NUMBER 1 1
$SM_VERSION 7
$SM_STANDARD_FIELD_SIZE 128 96
$SM_MICRON_MARKER 200µm
$SM_MICRON_BAR 300
$SM_PNU_HEIGHT 128
$SM_PNU_TYPE 1
$SM_NICKNAME IT200
$SM_DETECTOR SED
$SM_WD 11.6
$SM_SCAN_TIME 80
$SM_SCAN_TYPE 0
$SM_VACUUM_MODE HV
$SM_VACUUM 
$SM_SCAN_ROTATION 0
$SM_IMAGE_NUMBER 1971
$SM_DETECTOR1 SED
$SM_DETECTOR2 
$SM_DETECTOR3 
$SM_DETECTOR4 
$SM_DETECTOR1_ADD_RATIO 
$SM_DETECTOR2_ADD_RATIO 
$SM_DETECTOR3_ADD_RATIO 
$SM_DETECTOR4_ADD_RATIO 
$SM_INTEGRATION_NUMBER 1
$SM_SPECIMEN_TEMPERATURE 
$SM_PROBE_CURRENT 
$SM_GUN_VOLT 5.0
$SM_STAGE_BIAS_VOLT 0.0
$SM_COLUMN_MODE 0
$SM_MONITOR_MAGNIFICATION 141.4541015625
$MP_VERSION 5
$MP_GUN_TYPE W
$MP_CONTRAST1 1376
$MP_CONTRAST2 
$MP_CONTRAST3 
$MP_CONTRAST4 
$MP_BRIGHTNESS1 1844
$MP_BRIGHTNESS2 
$MP_BRIGHTNESS3 
$MP_BRIGHTNESS4 
$MP_BED_COMPO_SUPPRESS 
$MP_BED_SHADOW_SUPPRESS 
$MP_BED_GAIN 
$MP_BED_SHADOW_LEVEL 
$MP_PROBE_NUMBER 30.0
$MP_PROBE_CURRENT_MODE 0
$MP_BEAM_SHIFT 0 0
$MP_DYNAMIC_FOCUS 0
$MP_TILT_MAG_CORRECTION 0
$MP_STAGE_DRIVE 1 1 0 0 0 2
$MP_LOW_VACUUM_MODE 65535
$MP_FIELD_IMAGE_MAGNIFICATION 
