CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.5pl6/conf/instr/spect/uxnmr.info
Date         : Thu Aug 25 18:26:57 2022
Release      : TopSpin 3.5 pl 6
Installed in : C:/Bruker/TopSpin3.5pl6
Host         : CZC2222X54
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2533 MHz)
User         : nmrsu
System       : Avance III 700 NMR spectrometer
1H-frequency : 700.13 MHz
Description  : AVC700DB
Location     : Indian Institute of Science Education/Bhopal/India
Bruker Order : 10070595
Configured in: CZC2222X54:C:/Bruker/TopSpin3.5pl6/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.253
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/03005 ECL 06.02
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2
DRU2: AQS DRU-E Z102520/03004 ECL 06.02
- TCP/IP address = 149.236.99.88
- Firmware Version = 170619

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AW  R  5.1 REC-1  AQS RXAD1000 Z102118/351 ECL 05.01
     3   0x34 0xc9   0x1        X  1.3 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x29   0x8    AE  S  3.6 SGU-1  AQS SGU/2 1000 Z103082/01055 ECL 03.06 FPGA-Vs=AF
     6   0x11 0x52   0x4    AW  R  5.1 REC-2  AQS RXAD1000 Z102118/352 ECL 05.01
     7   0x25 0x29   0x8    AE  S  3.6 SGU-2  AQS SGU/2 1000 Z103082/01054 ECL 03.06 FPGA-Vs=AF
     8   0x26 0x29   0x8    AE  S  3.6 SGU-3  AQS SGU/2 1000 Z103082/01056 ECL 03.06 FPGA-Vs=AF
     9   0x27 0x29   0x8    AE  S  3.6 SGU-4  AQS SGU/2 1000 Z103082/01057 ECL 03.06 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0547 W1345093/0547 ECL 12:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0547 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2055 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6585 ECL 50
BLA_W1345097_0233 W1345097/0233 ECL 20:
- TCP/IP address = 149.236.99.251
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0233 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1564 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6686 ECL 50
BLA_W1345092_0561 W1345092/0561 ECL 11:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0561 ECL 11
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2044 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6616 ECL 50
LTRX Z109891/00063 ECL 01.02:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00063 ECL 01.02

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210212
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00063 ECL 01.02
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01047 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01197 ECL 01.03

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.253:/dev/tty01
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.253:/dev/tty04

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 1H19F (reflection meter)
                PN=Z103206, SN=01310 from 20220321
    Module  2 : 2H
                PN=Z003474, SN=00560 from 20220215
    Module  3 : XBB19F 2HS
                PN=Z003507, SN=00655 from 20120626
    Module  4 : XBB19F 2HS
                PN=Z003507, SN=00656 from 20120626
    Module  5 : 15N
                PN=Z003531, SN=00137 from 20120615
    Module  6 : 13C
                PN=Z003525, SN=00145 from 20120615



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0233 at TCP/IP 149.236.99.251)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0233 at TCP/IP 149.236.99.251)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0547 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0233 at TCP/IP 149.236.99.251)
SGU4 NORM output -> input 1 of transmitter 3 (BLAX300 E 6-365MHZ INR W1345092/0561 at TCP/IP 149.236.99.250)
SGU4 AUX  output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0233 at TCP/IP 149.236.99.251)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0547 at TCP/IP 149.236.99.252:
- amplifier X-500W uses blanking 3

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ BLAX300 E 6-365MHZ INR W1345097/0233 at TCP/IP 149.236.99.251:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 5

transmitter 3 = BLAX300 E 6-365MHZ INR W1345092/0561 at TCP/IP 149.236.99.250:
- amplifier X-300W uses blanking 4

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 700 Z109891/00063 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


