
New TopShim run:

version = topshim 2.1.0
date = 2022-08-30
time = 10:55:07.279
command = topshim 

FINE SHIMMING

Parameters:

probe = Z116098_0892
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 2.6 Hz, Target= 0.4 Hz, After= 0.6 Hz
Iteration 2: FWHM Before= 0.6 Hz, Target= 0.4 Hz, After= 0.8 Hz
Iteration 3: FWHM Before= 0.8 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 4: FWHM Before= 0.4 Hz, Target= 0.6 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, non-spinning) = 0.589

shim changes: 
Z	+79
Z2	+61
Z3	+38
Z4	-445
Z5	-248
Z6	+1472
Z7	+1233
Z8	+1257

duration = 1 min 2 sec
completed successfully
finished Tue Aug 30 10:56:07 2022


========================================================================
