
New TopShim run:

version = topshim 2.1.0
date = 2022-08-31
time = 08:05:28.975
command = topshim 

FINE SHIMMING

Parameters:

probe = Z116098_0892
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 0.8 Hz, Target= 0.7 Hz, After= 0.9 Hz
Iteration 2: FWHM Before= 0.9 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 3: FWHM Before= 0.5 Hz, Target= 0.5 Hz, After= 1.0 Hz
Iteration 4: FWHM Before= 1.0 Hz, Target= 0.5 Hz, After= 0.7 Hz
Iteration 5: FWHM Before= 0.7 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 6: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.8 Hz
Iteration 7: FWHM Before= 0.8 Hz, Target= 0.6 Hz, After= 0.8 Hz
Iteration 8: FWHM Before= 0.8 Hz, Target= 0.4 Hz, After= 1.3 Hz
Slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, non-spinning) = 0.607

shim changes: 
Z	+130
Z2	-25
Z3	-243
Z4	-460
Z5	+81
Z6	+1662
Z7	+1781
Z8	-154

duration = 1 min 55 sec
completed successfully
finished Wed Aug 31 08:07:22 2022


========================================================================
