
New TopShim run:

version = topshim 2.4.0
date = 2024-05-24
time = 11:38:49.519
command = topshim 

FINE SHIMMING

Parameters:

probe = Z125339_0021
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.5 Hz, After= 0.5 Hz
Iteration 3: FWHM Before= 0.5 Hz, Target= 0.5 Hz, After= 0.7 Hz
Iteration 4: FWHM Before= 0.7 Hz, Target= 0.5 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.474

shim changes: 
Z	-72
Z2	-35
Z3	+3
Z4	-79
Z5	+8

duration = 1 min 34 sec
completed successfully
finished Fri May 24 11:40:23 2024


========================================================================
