CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Wed Nov 17 15:39:38 2021
Release      : TopSpin 4.1.3
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.1.156.20210628
CPU          : Intel(R) Core(TM) i7-4700EQ CPU @ 2.40GHz (8 cores at 2034 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 400 NMR spectrometer
1H-frequency : 400.13 MHz
Description  : Avance Neo
Location     : Potsdam
Bruker Order : 416985
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- EPU/2: AV4 EPU/2 Embedded Processing Unit H153448F1/01334 ECL 01.04
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/04362 ECL 02.03
  Location: slot 1 in rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd2, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/04363 ECL 02.03
  Location: slot 2 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd11, DRX at /dev/bbu/drx4.5, RTD at /dev/bbu/rtd4.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/04364 ECL 02.03
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.22 via PCIe #5
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx5.5, RTD at /dev/bbu/rtd5.4
  Sequencer: FCube
  - FCube3
- GTU: AV4 GT-CONTROLLER UNIT Z148393/01374 ECL 01.02
  Location: slot 6 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20190906085855
  - Gradient resolution: 1.0 us
  Devices: MTD at /dev/mtd28, RTD at /dev/bbu/rtd9.4, GPROC at /dev/bbu/gproc9.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- PSM-A: AV4 PSM-A Z149510/01795 ECL 03.01
- HPPR/2 COVER2: HPPR/2 Cover2 Z124567/03432 ECL 00.05
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 1H19F (virtual 50 Ohm reference: 99.9%/0.2deg, reflection meter with CRP-Bias capability)
                  PN=Z103203, SN=01221 from 20200110
      Module  2 : 2H
                  PN=Z003471, SN=00696 from 20191129
      Module  3 : XBB19F 2HP
                  PN=Z106984, SN=00625 from 20191203
      Module  4 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111091, SN=00437 from 20191128
  
- HPLNA 1H19F: HPLNA 1H MODULE 400 Z103203/01221 ECL 06.04
- 2H: HPPR/2 2H MODULE 400 Z003471/00696 ECL 07.00
- XBB19F 2HP: HPPR/2 XBB19F 2HP MODULE 400 Z106984/00625 ECL 07.02
- HPLNA BB31P: HPLNA XBB 31P MODULE 400 Z111091/00437 ECL 04.04
- RACK: AV4 AQS CHASSIS Z149500/01418 ECL 02.00
- PSM-48V: AV4 PSM-48V Z149850/03049 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/01770 ECL 01.01
- FANTRAY: AV4 AQS FAN TRAY Z149501/01400 ECL 00.02
- REF 1200: AV4 REFERENCE 1200 Z148270/01497 ECL 02.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144055-000141 W144055/000141 ECL 01:
- TCP/IP address = 192.168.99.14
- Firmware VS    = 20201119
- Amplifier      = AV4 BLAH500 200-600: W144055/000141 ECL 01
- Controller     = BLA CONTROL BOARD 7: W133936/022257 ECL 21
BLA-W144059-000364 W144059/000364 ECL 10:
- TCP/IP address = 192.168.99.13
- Firmware VS    = 20201119
- Amplifier      = AV4 BLABB500 15-600: W144059/000364 ECL 10
- Controller     = BLA CONTROL BOARD 7: W133936/022886 ECL 21
BLA-W144059-000370 W144059/000370 ECL 10:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20201119
- Amplifier      = AV4 BLABB500 15-600: W144059/000370 ECL 10
- Controller     = BLA CONTROL BOARD 7: W133936/022284 ECL 21
LTRX Z109888/02927 ECL 04.01:
- TCP/IP address = 192.168.99.11
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 400: Z109888/02927 ECL 04.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11
- ELCB firmware version = 20210212
- ELCB = BSMS/2 ELCB: Z100818/08385 ECL 07.02
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- Shim System = BOSS3-SB
- SCB channels = 40
- Shim matrix file: 292722aa.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 Z7 Z8 XZ5 YZ5 (X2-Y2)Z3 (X2-Y2)Z4 (X2-Y2)Z5 XYZ3 XYZ4 XYZ5
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 400: Z109888/02927 ECL 04.01
- Lock: on L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/05449 ECL 05.04
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/01368 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: BACS2_H15000-01_1294
- TCP/IP address   = 192.168.98.3
- Protocol types   = SOAP

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 1 (AV4 BLAH500 200-600 W144055/000141 at TCP/IP 192.168.99.14)
TRX1 AUX  output -> input 1 of transmitter 4 (BSMS/2 LOCK TRANSCEIVER 400 Z109888/02927 at TCP/IP 192.168.99.11)
TRX2 NORM output -> input 1 of transmitter 3 (AV4 BLABB500 15-600 W144059/000370 at TCP/IP 192.168.99.12)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 2 (AV4 BLABB500 15-600 W144059/000364 at TCP/IP 192.168.99.13)
TRX3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLAH500 200-600 W144055/000141 at TCP/IP 192.168.99.14:
- amplifier 1H-500W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 2 = AV4 BLABB500 15-600 W144059/000364 at TCP/IP 192.168.99.13:
- amplifier B-500W uses blanking 3

transmitter 3 = AV4 BLABB500 15-600 W144059/000370 at TCP/IP 192.168.99.12:
- amplifier B-500W uses blanking 2

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 400 Z109888/02927 at TCP/IP 192.168.99.11:
- amplifier 2H-5W uses blanking 9


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 1H19F -> REC1
Tune-TRX1 -> 2H          -> REC1
Tune-TRX2 -> XBB19F 2HP  -> REC2
Tune-TRX3 -> HPLNA BB31P -> REC3
