EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
NAME		PULPROG
END
NAME		TD
END
NAME		NS
END
NAME		DS
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"sweep width in Hz"
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
                TEXT	"acquisition time"
END
NAME		RG
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3f usec"
		TEXT	"dwell time "
END
NAME		DE
		FORMAT	"%14.2f usec"
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
TEXT		"relaxation delay; 1-5 * T1"
END
T_NAME		d11
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d11=30m"
		INV_REL	"D[0]=d11"
		UNIT	"sec"
		TEXT	"d11=30m"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		DELTA
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"DELTA=d1-100m"
		INV_REL	"D[0]=DELTA"
		UNIT	"sec"
		TEXT	"DELTA=d1-100m"
		FORMAT	"%14.8f sec"
		NONEDIT
END
NAME		TD0
END
HEADER		"======== CHANNEL f1 ========"
NAME		NUC1
		NONEDIT
		TEXT	"nucleus for channel 1"
END
T_NAME		P1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P1=P[1]"
		INV_REL	"P[1]=P1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"f1 channel -  90 degree high power pulse"
END
T_NAME		PL1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL1=PL[1]"
		INV_REL	"PL[1]=PL1"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
TEXT		"f1 channel - power level for pulse (default)"
END
T_NAME		PL1W
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL1W=131*pow(10.0,(-6-PL[1])/10.0)"
		INV_REL	"PL[1]=-6-4.3425*log(PL1W/131)"
		UNIT	"no"
		FORMAT	"%14.8f W"
TEXT		"f1 channel - power level for pulse (default)"
END
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of observe channel"
END
HEADER		"======== CHANNEL f2 ========"
NAME		CPDPRG2
		TEXT	"file name for cpd2"
END
NAME		NUC2
		NONEDIT
		TEXT	"nucleus for channel 2"
END
T_NAME		PCPD2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0 1e38
		REL	"PCPD2=PCPD[2]"
		INV_REL	"PCPD[2]=PCPD2"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"f2 channel - 90 degree pulse for decoupling sequence"
END
T_NAME		PL2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL2=PL[2]"
		INV_REL	"PL[2]=PL2"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	"power PL2 "
END
T_NAME		PL12
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL12=PL[12]"
		INV_REL	"PL[12]=PL12"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
TEXT		"f2 channel - power level for CPD/BB decoupling"
END
T_NAME		PL13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL13=PL[13]"
		INV_REL	"PL[13]=PL13"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
TEXT		"f2 channel - power level for second CPD/BB decoupling"
END
T_NAME		PL2W
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL2W=35.2*pow(10.0,(-6-PL[2])/10.0)"
		INV_REL	"PL[2]=-6-4.3425*log(PL2W/35.2)"
		UNIT	"no"
		FORMAT	"%14.8f W"
		TEXT	"power PL2 in W"
END
T_NAME		PL12W
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL12W=35.2*pow(10.0,(-6-PL[12])/10.0)"
		INV_REL	"PL[12]=-6-4.3425*log(PL12W/35.2)"
		UNIT	"no"
		FORMAT	"%14.8f W"
TEXT		"f2 channel - power level for CPD/BB decoupling"
END
T_NAME		PL13W
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL13W=35.2*pow(10.0,(-6-PL[13])/10.0)"
		INV_REL	"PL[13]=-6-4.3425*log(PL13W/35.2)"
		UNIT	"no"
		FORMAT	"%14.8f W"
TEXT		"f2 channel - power level for second CPD/BB decoupling"
END
NAME		SFO2
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of observe channel"
END
