CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.7.0/conf/instr/spect/uxnmr.info
Date         : Wed Nov 12 17:16:55 2025
Release      : TopSpin 3.7.0
Installed in : C:/Bruker/TopSpin3.7.0
Host         : NMR-400
OS           : Windows 10 Enterprise 2015 LTSB (Vs 6.3)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v4 @ 3.50GHz (8 cores at 3492 MHz with Hyperthreading)
User         : nmradmin
System       : Avance III 400 NMR spectrometer
1H-frequency : 400.13 MHz
Description  : Avance III
Location     : O414
Bruker Order : 10015802
Configured in: NMR-400:C:/Bruker/TopSpin3.7.0/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.251
 - IPSO type: AQS
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : 1
- FREDs : none
- DPP : none

DRU1: AQS DRU Z100977/01364 ECL 06.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x72   0x4    AW  R  4.4 REC-1  AQS RXAD400 Z102116/1842 ECL 04.04
     3   0x34  0x2   0x1        X  5.2 REF-1  REF-400 Reference Board for AQS Receiver
     4   0x24 0x11   0x8    AE  S  2.6 SGU-1  AQS SGU/2 400 Z103080/02144 ECL 02.06 FPGA-Vs=AF
     5   0x25 0x11   0x8    AE  S  2.6 SGU-2  AQS SGU/2 400 Z103080/02145 ECL 02.06 FPGA-Vs=AF
    21   0x21 0xcf     0        P  0.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345083_0178 W1345083/0178 ECL 2:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH300/100 E 200-600MHZ INR: W1345083/0178 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0909 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/4709 ECL 05
- QNP-Accessory  : 1 X-input and 1 H-input
LTRX Z109888/00305 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 400: Z109888/00305 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20230420
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS1-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 400: Z109888/00305 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00015 ECL 01.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00031 ECL 01.00

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 1H (virtual 50 Ohm reference: 100.0%/0.1deg, reflection meter)
                PN=Z103203, SN=00043 from 20100420
    Module  2 : 1H/2H 1H (virtual 50 Ohm reference: 278.7%/83.3deg)
                PN=Z003959, SN=00765 from 20100416
    Module  3 : 1H/2H 2H (virtual 50 Ohm reference: 101.1%/-68.0deg)
                PN=Z003959, SN=00765 from 20100416
    Module  4 : XBB19F 2HS
                PN=Z003504, SN=00766 from 20100312



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH300/100 E 200-600MHZ INR W1345083/0178 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 1 of transmitter 2 (BSMS/2 LOCK TRANSCEIVER 400 Z109888/00305 at TCP/IP 149.236.99.20)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH300/100 E 200-600MHZ INR W1345083/0178 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH300/100 E 200-600MHZ INR W1345083/0178 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1

transmitter 2 = BSMS/2 LOCK TRANSCEIVER 400 Z109888/00305 at TCP/IP 149.236.99.20:
- amplifier 2H-5W uses blanking 7


Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
transmitter 1 = BLAXH300/100 E 200-600MHZ INR W1345083/0178 at TCP/IP 149.236.99.253:
- amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
- amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H


