[SemImageFile]
InstructName=SU8200
SemVersion=01-21
SDMVersion=
SerialNumber=8200-1539-02
DataNumber=SU8220 2178
SampleName=2
Format=tif
ImageName=2_2178.tif
Directory=D:\SEMdata\yuhao\20250603-2\
Date=06/03/2025
Time=11:47:53
Media=HD[Data]
DataSize=1280x960
PixelSize=4.960938
SignalName=SE(U)
DisplaySignalName=SE(U)
SEDetSetting=
AcceleratingVoltage=10000 Volt
DecelerationVoltage=0 Volt
DecelerationMode=
Magnification=20000
WorkingDistance=9395.55 um
EmissionCurrent=9800 nA
LensMode=Normal
PhotoSize=1000
MagnificationDisplay=0
Vacuum=
MicronMarker=2000
SubMagnification=0
SubSignalName=
SpecimenBias=0 V
Condencer1=5000
ScanSpeed=Capture_Rapid(32)
CaptureSpeed_Integration=
CalibrationScanSpeed=19
ImgEnhance=0
ColorMode=Grayscale
ColorPalette=
ScreenMode=Middle Screen
Comment=
KeyWord1=
KeyWord2=
Condition=Vacc=10.0kV   Mag=x20.0k   WD=9.4mm
DataDisplayCombine=1
StageType=5
StagePositionX=37653000
StagePositionY=27928000
StagePositionR=359.9
StagePositionZ=8000000
StagePositionT=0
FocusDepth=1.0
DynamicFocus=0
TiltCompensation=0
RasterRotation=-142.5
MagneticSample=OFF
EBIC_Value00=
EBIC_ValueFF=
EBIC_Polarity=
DriftCorrectionIntegration=0
