{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Housing","Pulser PCB","Power Supply"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Housing","index":0,"n_rows":35,"n_cols":16,"rows_kept":35,"cut":false,"hidden":false,"merged":[[8,0,8,5],[8,10,8,15],[8,8,8,9]],"flags":["formulas_cached_only"]}
["Merck - Scientific Engineering & Design"]
[]
[]
["Project Name:",null,"HTE Photoreactor"]
["Build Description:",null,"Housing"]
["BOM Version:",null,1]
["Quantity",null,1,{"$nulls":4},"Total  Project Cost"]
[{"$nulls":7},1777.26]
["Quantity Needed",{"$nulls":7},"Vendor Information",null,"Manufacturer/Designer Information"]
["Qty per Device","UOM","Total Qty","Qty per Pkg","Inventory Qty","Qty to Order","Cost per pkg","Total Cost","Vendor","Vendor Stock No","Mfr","Part/Drawing No","Description","Sub-Assembly","Modification Notes","Link"]
[1,"ea",1,1,null,1,270,270,"EMCO Industrial Plastics",null,null,"DVC20170154MP07A_Diffuser","Makrolon Lumen XT LC3 0.060\""]
[1,"ea",1,1,null,1,14,14,"Custom Thermoelectric",null,null,null,"Heat Sink 120mm Fan Bracket"]
[1,"ea",1,1,null,1,167,167,"Rotech Tool & Mold",null,null,"DVC20170154MP06A_BASE_PLATE","6061 Aluminum, Gray Anodized"]
[1,"ea",1,1,null,1,154,154,"Rotech Tool & Mold",null,null,"DVC20170154MP02A_LED_PLATE_NEST","6061 Aluminum, Gray Anodized"]
[1,"ea",1,1,null,1,280.6,280.6,"EMCO Industrial Plastics",null,null,"DVC20170154MA04B_Cover_Shield","2422 Orange Tint Acrylic, Solvent Welded"]
[1,"ea",1,1,null,1,null,0,"Xometry",null,null,"MKW20170154MP14B Cable Pass Through A","MJF Nylon 12"]
[1,"ea",1,1,null,1,null,0,"Xometry",null,null,"MKW20170154MP15B Cable Pass Through B","MJF Nylon 12"]
[1,"ea",1,1,null,1,131,131,"Mcmaster-Carr","9936K13",null,null,"Control Cable Seven 20-Gauge Wires, 100 ft. Length"]
[1,"ea",1,1,null,1,82,82,"Mcmaster-Carr","9936K17",null,null,"Control CableThree 18-Gauge Wires"]
[1,"ea",1,1,null,1,22.62,22.62,"Mouser",null,"Mean Well","709-GSM60A24-P1J","Desktop AC Adapters 60W 24V 2.5A Medical Power Supply"]
[1,"ea",1,1,null,1,41.14,41.14,"Mouser",null,"Sanyo","9GA1224P4G001","DC Fans DC Fan, 120x25mm, 24VDC, 134CFM, 11.28W, 57dBA, 6400RPM, Low Power Consumption, Ribbed, Tachometer, PWM"]
[1,"ea",1,1,null,1,9.73,9.73,"Mouser",null,"Souriau","UTG1128S","Standard Circular Connector 8P Socket Receptacle Cable Mount Size 12"]
[1,"ea",1,1,null,1,12.19,12.19,"Mouser",null,"Souriau","UTG610-4PN","Standard Circular Connector 4P Straight Pin Plug Shell Size 10"]
[null,"ea",0,1,null,0,2.48,0,"Mcmaster-Carr","93330A563",null,null,"Female Threaded Round Standoff, Aluminum, 1/4\" OD, 4\" Long, 8-32 Thread",null,"turn down length to 3.750\""]
[1,"ea",1,1,null,1,15.83,15.83,"Mouser",null,"Souriau","UTG10AC","Shell Size 10 Cable Clamp"]
[2,"ea",2,1,null,2,6.08,12.16,"Mouser",null,"Souriau","UTG12AC","Shell Size 12 Cable Clamp"]
[1,"ea",1,1,null,1,12.41,12.41,"Mouser",null,"Souriau","UTG1128P","Standard Circular Connector 8P Pin Receptacle Cable Mount Size 12"]
[7,"ea",7,1,null,7,4.52,31.639999999999997,"Mouser",null,"Souriau","RM20M12D28","Standard Circular Contacts MACHINED PIN 22-20"]
[3,"ea",3,1,null,3,3.54,10.620000000000001,"Mouser",null,"Souriau","RM16M23D28","Standard Circular Contacts MACHINED PIN 20-16"]
[7,"ea",7,1,null,7,5,35,"Mouser",null,"Souriau","RC20M12D28","Standard Circular Contacts Crimp Socket Contact 20-22 AWG"]
[3,"ea",3,1,null,3,4.45,13.350000000000001,"Mouser",null,"Souriau","RC16M23D28","Standard Circular Contacts Crimp Socket Contact 16-20 AWG"]
[1,"ea",1,1,null,1,7.5,7.5,"Rotech",null,null,"DVC20170154MP01A_LED_BOARD","6061 Aluminum, Gray Anodized"]
[48,"ea",48,1,null,48,8.99,431.52,"Kiwi Lighting",null,null,null,"20W Cree XTE XT-E 4Leds Led Emitter Lamp Light On 20MM Copper PCB Board"]
[1,"ea",1,1,null,1,22.95,22.95,"Custom Thermoelectric",null,null,"HS-5.4-5.4-1.4-01","Heat Sink 5.4 x 5.4 x 1.4\""]
[null,"ea",0,1,null,0,58,0,"Rotech",null,null,"DVC20170154MP03A_Heat_Sink","HS-5.4-5.4-1.4-01 modification"]

{"sheet":"Pulser PCB","index":1,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[[8,0,8,5],[8,8,8,9],[8,10,8,15]],"flags":["formulas_cached_only"]}
["Merck - Scientific Engineering & Design"]
[]
[]
["Project Name:",null,"HTE Photoreactor"]
["Build Description:",null,"Pulser"]
["BOM Version:",null,1]
["Quantity",null,1,{"$nulls":4},"Total  Project Cost"]
[{"$nulls":7},34.07]
["Quantity Needed",{"$nulls":7},"Vendor Information",null,"Manufacturer/Designer Information"]
["Qty per Device","UOM","Total Qty","Qty per Pkg","Inventory Qty","Qty to Order","Cost per pkg","Total Cost","Vendor","Vendor Stock No","Mfr","Part/Drawing No","Description","Sub-Assembly","Modification Notes","Link"]
[1,"ea",1,1,null,1,25,25,null,null,null,"MKW20180126CA01A.kicad_pcb","0.0625\" FR4 PCB"]
[1,"ea",1,1,null,1,null,null,"Xometry",null,null,"MKW20170154MP101A Back Cover","FDM Black ASA"]
[1,"ea",1,1,null,1,null,null,"Xometry",null,null,"MKW20170154MP102A Bottom Cover","FDM Black ASA"]
[1,"ea",1,1,null,1,null,null,"Xometry",null,null,"MKW20170154MP103A Front Cover","FDM Black ASA"]
[1,"ea",1,1,null,1,2.14,null,"Mouser",null,"Amphenol","031-5431-10RFX","RF Connectors / Coaxial Connectors PC R/A BLHD JCK Ni WHITE HOUSING"]
[1,"ea",1,1,null,1,1.95,null,"Mouser",null,"Deltron","571-0500","Test Sockets SINGLE PCB SOCK RED"]
[1,"ea",1,1,null,1,1.49,null,"Mouser",null,"Deltron","571-0100","Test Sockets SINGLE PCB SOCK BLK"]
[1,"ea",1,1,null,1,2.02,null,"Mouser",null,"Deltron","571-0400","Test Sockets 4MM SINGLE SKT GREEN"]
[2,"ea",2,1,null,2,null,null,"Mouser",null,null,"IRLB4030PBF"]
[1,"ea",1,1,null,1,null,null,"Mouser",null,null,null,"4.7k 0805 Resistor"]
[2,"ea",2,1,null,2,null,null,"Mouser",null,null,null,"10u 0805 Ceramic Capacitor"]
[1,"ea",1,1,null,1,null,null,"Mouser",null,null,null,"10R0 0805 Resistor"]
[1,"ea",1,1,null,1,null,null,"Mouser",null,"Keystone",4527,"5x20 fuseholder"]
[1,"ea",1,1,null,1,null,null,"Mouser",null,"Norcomp","182-009-113R561","DB9M Right Angle Connector"]
[1,"ea",1,1,null,1,null,null,"Mouser",null,"TI","UCC37322D","MOSFET Power Driver 9A, 4  15 V, Non-Inverting, 8-Pin SOIC"]
[1,"ea",1,1,null,1,9.07,9.07,"Mouser",null,"Souriau","UTG010-4S","Standard Circular Connector 4P Socket Receptacle Wall Mount Size 10"]

{"sheet":"Power Supply","index":2,"n_rows":15,"n_cols":16,"rows_kept":15,"cut":false,"hidden":false,"merged":[[8,0,8,5],[8,8,8,9],[8,10,8,15]],"flags":["formulas_cached_only"]}
["Merck - Scientific Engineering & Design"]
[]
[]
["Project Name:",null,"HTE Photoreactor"]
["Build Description:",null,"Power Supply"]
["BOM Version:",null,1]
["Quantity",null,1,{"$nulls":4},"Total  Project Cost"]
[{"$nulls":7},341.12]
["Quantity Needed",{"$nulls":7},"Vendor Information",null,"Manufacturer/Designer Information"]
["Qty per Device","UOM","Total Qty","Qty per Pkg","Inventory Qty","Qty to Order","Cost per pkg","Total Cost","Vendor","Vendor Stock No","Mfr","Part/Drawing No","Description","Sub-Assembly","Modification Notes","Link"]
[1,"ea",1,1,null,1,341.12,341.12,"Mouser",null,"BK",9111,"180W Multi Range 60V/8A DC Power Supply"]
[1,null,null,1,null,null,99.99,null,"Amazon",null,null,null,"Koolertron Upgraded 15MHz DDS Signal Generator Counter,High Precision Dual-channel Arbitrary Waveform Function Generator Frequency Meter 200MSa/s (15M"]
[6,null,null,24,null,null,18.99,null,"Amazon",null,null,null,"WGGE WG-3333 24k Gold Plated Speaker Banana Plugs-Closed Screw Type (12 Pairs (24 Plugs))"]
[3,null,null,1,null,null,0.78,null,"Mcmaster-Carr","95947A727",null,null,"Aluminum Female Threaded Hex Standoff"]
[{"$nulls":6},4.86,null,"Amazon",null,null,null,"StarTech.com 0.5m Black Straight Through DB9 RS232 Serial Cable - DB9 RS232 Serial Extension Cable - Male to Female Cable - 50cm"]