{"text_format":"2","workbook":"xls","n_sheets":6,"sheets":["Summa data","BZC data","TWA-E BZC Ratio","Median GSD","RA","Acute 10"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Summa data","index":0,"n_rows":81,"n_cols":11,"rows_kept":81,"cut":false,"hidden":false,"merged":[[0,2,0,4],[0,5,0,7]],"flags":["formulas_cached_only"]}
[null,null,"Engine fire",null,null,"Cabin fire"]
[null,"Time(min)",0.5,2,2,0.5,2,3]
[null,null,"Startup","Knock","Over","Startup","Knock","Over"]
[null,null,"SMA-1","SMA-2","SMA-3","SMA-4","SMA-5","SMA-6","TWA-E","TWA-E"]
["Entry","Compound","µg/m3","µg/m3","µg/m3","µg/m3","µg/m3","µg/m3","ug/m3","mg/m3","MW"]
[2,"Dichlorodifluromethane (CFC12)",5100,2400,48000,null,null,5.9,10336.77,10.33677,86.47]
[33,"Benzene",5200,1600,11000,60000,1400,380,6174,6.174,78.11]
[46,"Toluene",1400,9300,3800,10000,4600,950,4395,4.395,92.13]
[1,"Propene",3300,910,11000,18000,1400,160,3775,3.775]
[57,"Styrene",830,3300,1600,14000,2300,450,2316.5,2.3165,104.16]
[12,"Acetone",400,840,3800,12000,1900,300,2018,2.018,58.05]
[55,"m,p,o-Xylenes",250,6200,970,770,2000,330,2842,2.842,106.16]
[15,"Acrylonitrile",320,null,770,27000,380,66,1615.8,1.6158,53.05]
[6,"1,3-Butadiene",2300,400,4800,6800,250,49,1559.7,1.5597,54.09]
[74,"Naphthalene",2400,930,1200,10000,600,170,1217,1.217,128.19]
[11,"Acrolein",560,350,1400,15000,180,48,1178.4,1.1784000000000001,56.06]
[66,"1,2,4-Trimethylbenzene",70,4200,380,150,700,100,1097,1.097,120.19]
[10,"Acetonitrile",280,120,700,14000,120,34,912.2,0.9122,41.05]
[3,"Chloromethane (methyl chloride)",330,170,1200,11000,190,46,892.3,0.8923,50.49]
[54,"Ethylbenzene",150,2200,410,1400,700,120,775.5,0.7755,106.16]
[28,"n-Hexane",29,1100,300,150,1500,310,681.95,0.6819500000000001,86.18]
[41,"n-Heptane",21,870,210,110,840,180,444.55,0.44455,100.2]
[31,"1,2-Dichloroethane",null,null,1100,480,670,140,420,0.42,96.95]
[64,"4-Ethyltoluene",27,1400,120,160,220,32,366.95,0.36695]
[65,"1,3,5-Trimethylbenzene",32,1400,120,null,210,31,356.9,0.3569,120.2]
[9,"Ethanol",400,720,670,null,null,null,298,0.298,46.07]
[40,"Methyl Methacrylate",440,170,210,330,810,58,293.9,0.2939,100.13]
[51,"n-Octane",24,670,150,97,310,61,250.35,0.25035,114.22]
[63,"n-Propylbenzene",21,900,93,170,150,24,245.35,0.24534999999999998]
[5,"Vinyl Chloride",43,null,120,3700,74,12,229.55,0.22955,62.5]
[59,"n-Nonane",21,540,98,140,140,21,169.95,0.16995,128.26]
[25,"2-Butanone (MEK)",51,160,210,1100,71,18,151.15,0.15115,72.1]
[14,"2-Propanol (Isopropyl Alcohol)",50,52,350,null,280,19,144.6,0.1446,60.09]
[30,"Tetrahydrofuran (THF)",null,280,360,160,null,null,136,0.136,72.1]
[8,"Chloroethane (ethyl chloride)",100,38,150,620,220,28,126,0.126,64.5]
[18,"3-Chloro-1-propene (Allyl Chloride)",null,null,240,550,100,31,104.8,0.10479999999999999,76.5]
[39,"1,4-Dioxane",21,160,130,130,160,13,101.45,0.10145,88.1]
[71,"d-Limonene",null,290,210,null,null,null,100,0.1]
[35,"Cyclohexane",null,190,null,null,220,48,96.4,0.0964,82.14]
[24,"Vinyl Acetate",null,null,null,1500,null,55,91.5,0.0915,86.09]
[61,"Cumene",null,250,null,130,76,11,75,0.075,120.19]
[50,"n-Butyl Acetate",{"$nulls":4},350,8.7,72.61,0.07261,116.16]
[53,"Chlorobenzene",38,37,58,910,null,null,66.4,0.0664,112.56]
[67,"Benzyl Chloride",null,64,180,320,null,null,64.8,0.0648,126.58]
[20,"Carbon Disulfide",67,72,110,200,40,7.2,59.910000000000004,0.059910000000000005,76.14]
[36,"1,2-Dichloropropane (propylene dichloride)",{"$nulls":4},170,49,48.7,0.0487,113]
[43,"4-Methyl-2-pentanone (hexone)",null,81,50,null,null,null,26.2,0.026199999999999998,100.2]
[47,"2-Hexanone (methyl n-butyl ketone)",26,null,null,230,null,null,12.8,0.0128,100.2]
[17,"Methylene Chloride (dichloromethane)",null,null,null,250,null,null,12.5,0.0125,84.9]
[7,"Bromomethane (methyl bromide)",null,null,null,140,null,null,7,0.007,95]
[null,"Carbon monoxide",{"$nulls":7},0,28.01]
[null,"Formaldehyde",{"$nulls":7},0]
[4,"1,2-Dichloro-1,1,2,2-tetrafluoroethane (CFC 114)",{"$nulls":6},0,0]
[13,"Trichlorofluoromethane",{"$nulls":6},0,0]
[16,"1,1-Dichloroethene",{"$nulls":6},0,0]
[19,"Trichlorotrifluoroethane",{"$nulls":6},0,0]
[21,"trans-1,2-Dichloroethene",{"$nulls":6},0,0]
[22,"1,1-Dichloroethane",{"$nulls":6},0,0]
[23,"Methyl tert-Butyl Ether",{"$nulls":6},0,0]
[26,"cis-1,2-Dichloroethene",{"$nulls":6},0,0]
[27,"Ethyl Acetate",{"$nulls":6},0,0]
[29,"Chloroform",{"$nulls":6},0,0]
[32,"1,1,1-Trichloroethane",{"$nulls":6},0,0]
[34,"Carbon Tetrachloride",{"$nulls":6},0,0]
[37,"Bromodichloromethane",{"$nulls":6},0,0]
[38,"Trichloroethene",{"$nulls":6},0,0]
[42,"cis-1,3-Dichloropropene",{"$nulls":6},0,0]
[44,"trans-1,3-Dichloropropene",{"$nulls":6},0,0]
[45,"1,1,2-Trichloroethane",{"$nulls":6},0,0]
[48,"Dibromochloromethane",{"$nulls":6},0,0]
[49,"1,2-Dibromoethane",{"$nulls":6},0,0]
[52,"Tetrachloroethene",{"$nulls":6},0,0]
[56,"Bromoform",{"$nulls":6},0,0]
[60,"1,1,2,2-Tetrachloroethane",{"$nulls":6},0,0]
[62,"alpha-Pinene",{"$nulls":6},0,0]
[68,"1,3-Dichlorobenzene",{"$nulls":6},0,0]
[69,"1,4-Dichlorobenzene",{"$nulls":6},0,0]
[70,"1,2-Dichlorobenzene",{"$nulls":6},0,0]
[72,"1,2-Dibromo-3-chloropropane",{"$nulls":6},0,0]
[73,"1,2,4-Trichlorobenzene",{"$nulls":6},0,0]
[75,"Hexachlorobutadiene",{"$nulls":6},0,0]

{"sheet":"BZC data","index":1,"n_rows":11,"n_cols":9,"rows_kept":11,"cut":false,"hidden":false,"merged":[[1,0,1,8],[10,0,10,8]],"flags":["formulas_cached_only"]}
[]
["Table 2  Summary of 15-min TWA BZCs (mg m–3) measured during the suppression of three separate vehicle fires."]
["Compound","N","Non-detectsa","Min ","Max ","GM ","GSD","X95","Lowest STEL or ceiling limit (C) (mg m–3)"]
["Benzene",12,8,"<0.21",0.33,0.2,1.5,0.38,"3.2 Ce"]
["Ethyl benzene",12,10,"<0.14",0.33,0.052,3.1,0.33,"545e,f"]
["Toluene",12,1,"<0.17",13,0.9,4.8,12,"560e"]
["Xylenes",12,10,"<0.34",0.56,0.26,1.5,0.52,"655e,f"]
["Formaldehyde",12,7,"<0.14",0.67,0.11,2.5,0.52,"0.12 Ce"]
["COb",12,0,0.03,25,3.3,6.2,65,"230 Ce"]
["TRIGc","10d",7,"<0.018",0.03,0.017,1.3,0.027,"0.044g"]
["a Values below the minimum detectable concentration were assigned values using maximum likelihood estimation. b Average CO concentration for the engine and cabin fires combined (~10 min of sampling time). c TRIG concentrations measured during cabin fire suppression only. d Two TRIG samples were excluded due to sampling pump error. e NIOSH REL. f ACGIH TLV. g Sweden OEL."]

{"sheet":"TWA-E BZC Ratio","index":2,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"VP","TWA-E","GM PBZ","Ratio"]
["Benzene",75,6.17,0.2,0.03241491085899514]
["Toluene",21,4.39,0.9,0.2050113895216401]
["m,p,o-Xylenes",9,2.84,0.26,0.09154929577464789]
["Ethylbenzene",7,0.78,0.052,0.06666666666666667]
[null,null,null,"Mean",0.09891056570548745]
[null,null,null,"STDEV",0.07477279863727283]
[null,null,null,"Median",0.07910798122065728]

{"sheet":"Median GSD","index":3,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[[16,0,16,5]],"flags":["formulas_cached_only"]}
[null,"IHDA","IHDA",null,"GSD"]
[null,"GM","GSD","NDs","Exclude <30% detection rate"]
["Toluene",0.9,4.8,1,4.8]
["Xylene",0.26,1.5,10]
["Benzene",0.2,1.5,8,1.5]
["Ethyl benzene",0.052,3.1,10]
["Formaldehyde",0.11,2.5,7,2.5]
["TRIG",0.017,1.3,7,1.3]
["CO**",5.6,5.7,0]
[null,null,null,"Mean",2.5250000000000004]
[null,null,null,"STDEV",1.604940289647353]
[null,null,null,"Median",2]
[]
[]
[]
[]
["**CO not inlcuded because inorganic and short term direct reading samples may not be directly comparable with the 15-min TWA "]

{"sheet":"RA","index":4,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,8,0,9],[0,10,0,11],[0,4,0,5]],"flags":["formulas_cached_only"]}
[null,null,"Measured BZC",null,"Measured or predicted BZC",null,null,null,"HQ analysis by GM",null,"HQ analysis by X95"]
["Compound","TWA-E","GM","X95","GM","X95","OEL mg/m3","STEL mg/m3","by OEL*","by STEL","by OEL*","by STEL","Lowest OEL","Lowest STEL"]
["Formaldehyde",null,null,null,0.11,0.52,2.5,0.12,0.001375,0.9166666666666667,0.006500000000000001,4.333333333333334,"OSHA","NIOSH (ceiling)"]
["Acrolein",1.1784000000000001,null,null,0.09427200000000001,0.9768483318956992,0.25,0.25,0.011784000000000001,0.37708800000000003,0.1221060414869624,3.907393327582797,"NIOSH","ACGIH"]
["TRIG",null,null,null,0.017,0.027,0.02,0.044,0.026562500000000003,0.3863636363636364,0.042187499999999996,0.6136363636363636,"Sweden, UK-HSE","Sweden"]
["Carbon monoxide",null,null,null,3.3,65,29,229,0.0035560344827586204,0.014410480349344978,0.07004310344827586,0.2838427947598253,"ACGIH","NIOSH (ceiling)"]
["Benzene",6.174,0.2,0.38,0.2,0.38,0.32,3.2,0.01953125,0.0625,0.037109375,0.11875,"NIOSH","NIOSH"]
["1,3-Butadiene",1.5597,null,null,0.12477600000000001,1.2929313842988137,2.2,11,0.0017723863636363636,0.011343272727272728,0.018365502617880874,0.11753921675443761,"OSHA","OSHA"]
["Acrylonitrile",1.6158,null,null,0.129264,1.3394361292235832,2.2,22,0.0018361363636363634,0.005875636363636363,0.019026081381016805,0.060883460419253785,"NIOSH","NIOSH (ceil), OSHA"]
["1,2-Dichloroethane",0.42,null,null,0.0336,0.3481638657469396,4,8,0.0002625,0.0042,0.0027200302011479655,0.04352048321836745,"NIOSH","NIOSH"]
["1,4-Dioxane",0.10145,null,null,0.008116,0.08409815280958816,72,3.6,3.5225694444444446e-06,0.0022544444444444443,3.650093437916153e-05,0.023360598002663376,"ACGIH","NIOSH (ceil)"]
["Toluene",4.395,0.9,11.7,0.9,11.7,75,560,0.000375,0.0016071428571428571,0.004875,0.02089285714285714,"ACGIH ","NIOSH"]
["Vinyl Chloride",0.22955,null,null,0.018364000000000002,0.19028813186240476,2.5,12,0.00022955000000000002,0.0015303333333333334,0.0023786016482800596,0.015857344321867063,"ACGIH, OSHA","OSHA"]
["3-Chloro-1-propene (Allyl Chloride)",0.10479999999999999,null,null,0.008383999999999999,0.08687517411971254,3,6,8.733333333333332e-05,0.0013973333333333331,0.0009049497304136723,0.014479195686618757,"ACGIH, NIOSH, OSHA","ACGIH, NIOSH"]
["Naphthalene",1.217,null,null,0.09736,1.008846249081013,50,75,6.0849999999999995e-05,0.0012981333333333333,0.0006305289056756331,0.013451283321080174,"ACGIH, NIOSH, OSHA","ACGIH, NIOSH"]
["Styrene",2.3165,null,null,0.18532,1.9202895119113945,85,170,6.813235294117648e-05,0.0010901176470588237,0.000705988791143895,0.01129582065830232,"ACGIH","ACGIH"]
["Benzyl Chloride",0.0648,null,null,0.005184,0.053716710715242116,5,5,3.24e-05,0.0010368,0.00033572944197026323,0.010743342143048423,"ACGIH, OSHA","NIOSH"]
["Vinyl Acetate",0.0915,null,null,0.00732,0.07584998503772614,35,14,6.535714285714287e-06,0.0005228571428571428,6.77232009265412e-05,0.005417856074123296,"ACGIH","NIOSH (ceil)"]
["Chloromethane (methyl chloride)",0.8923,null,null,0.071384,0.7396824223952243,105,205,2.1245238095238093e-05,0.00034821463414634146,0.00022014357809381675,0.0036082069385132893,"ACGIH","ACGIH"]
["Carbon Disulfide",0.059910000000000005,null,null,0.004792800000000001,0.04966308856404561,3,30,4.992500000000001e-05,0.00015976000000000003,0.0005173238392088083,0.001655436285468187,"ACGIH, NIOSH","NIOSH"]
["Acetone",2.018,null,null,0.16144,1.6728444787555337,590,1780,8.550847457627119e-06,9.069662921348314e-05,8.86040507815431e-05,0.000939800268963783,"NIOSH","ACGIH"]
["m,p,o-Xylenes",2.842,0.26,0.52,0.26,0.52,435,655,1.8678160919540232e-05,0.0003969465648854962,3.7356321839080464e-05,0.0007938931297709924,"ACGIH, NIOSH, OSHA","ACGIH, NIOSH"]
["Ethylbenzene",0.7755,0.052,0.33,0.052,0.33,435,545,3.735632183908046e-06,9.541284403669724e-05,2.370689655172414e-05,0.0006055045871559634,"ACGIH, NIOSH, OSHA","ACGIH, NIOSH"]
["Methyl Methacrylate",0.2939,null,null,0.023512,0.24363180986434657,205,410,3.5841463414634147e-06,5.7346341463414635e-05,3.713899540615039e-05,0.0005942239264984063,"ACGIH","ACGIH"]
["Tetrahydrofuran (THF)",0.136,null,null,0.01088,0.1127387755751995,150,300,2.266666666666667e-06,3.626666666666667e-05,2.3487244911499894e-05,0.0003757959185839983,"ACGIH","ACGIH"]
["2-Hexanone (methyl n-butyl ketone)",0.0128,null,null,0.0010240000000000002,0.010610708289430542,4,40,8.000000000000001e-06,2.5600000000000006e-05,8.289615851117611e-05,0.00026526770723576357,"NIOSH","ACGIH"]
["n-Heptane",0.44455,null,null,0.035564,0.36851487266143335,350,1800,3.1753571428571426e-06,1.9757777777777778e-05,3.290311363048512e-05,0.00020473048481190742,"NIOSH","NIOSH (ceil)"]
["2-Butanone (MEK)",0.15115,null,null,0.012092,0.12529754358964268,590,885,6.404661016949153e-07,1.3663276836158192e-05,6.636522435892091e-06,0.00014157914529903126,"ACGIH, NIOSH, OSHA","ACGIH, NIOSH"]
["Ethanol",0.298,null,null,0.02384,0.24703055236330476,1900,1900,3.921052631578948e-07,1.2547368421052631e-05,4.0630025059754075e-06,0.00013001608019121304,"NIOSH, OSHA","ACGIH"]
["2-Propanol (Isopropyl Alcohol)",0.1446,null,null,0.011568,0.11986784520716064,490,985,7.377551020408163e-07,1.1744162436548224e-05,7.64463298515055e-06,0.00012169324386513771,"ACGIH","ACGIH"]
["n-Octane",0.25035,null,null,0.020028,0.20753053283272938,350,1800,1.7882142857142859e-06,1.1126666666666666e-05,1.852951186006512e-05,0.00011529474046262744,"NIOSH","NIOSH"]
["4-Methyl-2-pentanone (hexone)",0.026199999999999998,null,null,0.0020959999999999998,0.021718793529928136,205,300,3.195121951219512e-07,6.986666666666666e-06,3.3107916966353866e-06,7.239597843309378e-05,"NIOSH","NIOSH"]
["n-Butyl Acetate",0.07261,null,null,0.005808799999999999,0.06019090069496496,710,950,2.5566901408450703e-07,6.114526315789473e-06,2.649247389743176e-06,6.335884283680522e-05,"ACGIH, NIOSH, OSHA","ACGIH, NIOSH"]
["Methylene Chloride (dichloromethane)",0.0125,null,null,0.001,0.010362019813897012,85,435,3.6764705882352943e-07,2.2988505747126437e-06,3.809566108050372e-06,2.382073520436095e-05,"OSHA","OSHA"]
["Acetonitrile",0.9122,null,null,0.072976,0.7561787579389484,34,0,6.707352941176471e-05,null,0.0006950172407527099,null,"ACGIH, NIOSH"]
["1,2,4-Trimethylbenzene",1.097,null,null,0.08776,0.9093708588676018,125,0,2.194e-05,null,0.00022734271471690047,null,"ACGIH, NIOSH "]
["n-Hexane",0.6819500000000001,null,null,0.05455600000000001,0.5653103529669654,180,0,9.47152777777778e-06,null,9.814415850120927e-05,null,"ACGIH, NIOSH"]
["1,3,5-Trimethylbenzene",0.3569,null,null,0.028552,0.2958563897263875,125,0,7.138e-06,null,7.396409743159687e-05,null,"ACGIH, NIOSH"]
["Dichlorodifluromethane (CFC12)",10.33677,null,null,0.8269415999999999,8.568785244135697,4950,null,5.220590909090909e-06,null,5.40958664402506e-05,null,"ACGIH, NIOSH, OSHA"]
["Bromomethane (methyl bromide)",0.007,null,null,0.0005600000000000001,0.005802731095782328,4,0,4.3750000000000005e-06,null,4.5333836685799434e-05,null,"ACGIH"]
["Chlorobenzene",0.0664,null,null,0.005312,0.05504304925142093,46,0,3.608695652173913e-06,null,3.739337585015009e-05,null,"ACGIH"]
["1,2-Dichloropropane (propylene dichloride)",0.0487,null,null,0.003896,0.04037042919494276,46,0,2.646739130434783e-06,null,2.7425563311781768e-05,null,"ACGIH"]
["Chloroethane (ethyl chloride)",0.126,null,null,0.01008,0.10444915972408189,260,0,1.2115384615384616e-06,null,1.2553985543759842e-05,null,"ACGIH"]
["Cumene",0.075,null,null,0.006,0.062172118883382074,245,0,7.653061224489796e-07,null,7.930117204513019e-06,null,"ACGIH, NIOSH, OSHA"]
["n-Nonane",0.16995,null,null,0.013595999999999999,0.14088202138974376,1050,0,4.046428571428571e-07,null,4.192917303266183e-06,null,"ACGIH, NIOSH"]
["Cyclohexane",0.0964,null,null,0.007712,0.07991189680477376,1050,null,2.2952380952380952e-07,null,2.378330262046838e-06,null,"ACGIH, NIOSH, OSHA"]
["4-Ethyltoluene",0.36695,null,null,0.029356,0.3041874536567607,0,0]
["d-Limonene",0.1,null,null,0.008,0.0828961585111761,0,0]
["n-Propylbenzene",0.24534999999999998,null,null,0.019628,0.20338572490717055,0,0]
["Propene",3.775,null,null,0.302,3.1293299837968975,0,0]
[{"$nulls":7},"HI for all compounds",0.06779087869199582,1.7904793375381682,0.330388632465993,9.604108295068238]
[]
["*assumes 15 min exposure, with 0 exposure for rest of 8 hours"]

{"sheet":"Acute 10","index":5,"n_rows":24,"n_cols":18,"rows_kept":24,"cut":false,"hidden":false,"merged":[[5,12,5,16],[5,2,5,3],[5,4,5,5]],"flags":["formulas_cached_only"]}
["Supplementary Material (ESI) for Journal of Environmental Monitoring"]
["This journal is © The Royal Society of Chemistry 2011"]
[]
[]
[]
[null,null,"Measured BZC",null,"Measured or predicted BZC",{"$nulls":7},"Target organ for acute health effects"]
["Compound","TWA-E","GM","X95","GM","X95","OEL mg/m3","STEL mg/m3","HQ analysis by GM","HQ analysis by X95","Lowest OEL","Lowest STEL","Respiratory tract","Eyes","Central nervous system","Liver/ kidney","Blood","Human Carcinogen"]
["Formaldehyde",null,null,null,0.11,0.52,2.5,0.12,0.9166666666666667,4.333333333333334,"OSHA","NIOSH (ceiling)","X","X",null,null,null,"Reasonably anticipated"]
["Acrolein",1.1784000000000001,null,null,0.09427200000000001,0.9768483318956992,0.25,0.25,0.37708800000000003,3.907393327582797,"NIOSH","ACGIH","X","X"]
["TRIG",null,null,null,0.017,0.027,0.02,0.044,0.3863636363636364,0.6136363636363636,"Sweden, UK-HSE","Sweden","X","X"]
["Carbon monoxide",null,null,null,3.3,65,29,229,0.014410480349344978,0.2838427947598253,"ACGIH","NIOSH (ceiling)","X",null,null,null,"X"]
["Benzene",6.174,0.2,0.38,0.2,0.38,0.32,3.2,0.0625,0.11875,"NIOSH","NIOSH","X","X","X",null,null,"Known"]
["1,3-Butadiene",1.5597,null,null,0.12477600000000001,1.2929313842988137,2.2,11,0.011343272727272728,0.11753921675443761,"OSHA","OSHA","X","X","X",null,null,"Known"]
["Acrylonitrile",1.6158,null,null,0.129264,1.3394361292235832,2.2,22,0.005875636363636363,0.060883460419253785,"NIOSH","NIOSH (ceil), OSHA","X","X","X",null,null,"Reasonably anticipated"]
["1,2-Dichloroethane",0.42,null,null,0.0336,0.3481638657469396,4,8,0.0042,0.04352048321836745,"NIOSH","NIOSH","X","X","X","X",null,"Reasonably anticipated"]
["1,4-Dioxane",0.10145,null,null,0.008116,0.08409815280958816,72,3.6,0.0022544444444444443,0.023360598002663376,"ACGIH","NIOSH (ceil)","X","X",null,null,null,"Reasonably anticipated"]
["Toluene",4.395,0.9,11.7,0.9,11.7,75,560,0.0016071428571428571,0.02089285714285714,"ACGIH ","NIOSH","X","X","X"]
[{"$nulls":11},"HI by GM",1.7823092797721445,1.7678987994227995,0.08552605194805195,0.0042,0.014410480349344978]
[{"$nulls":11},"HI by X95",9.5231524348499,9.239309640090074,0.361586017534916,0.04352048321836745,0.2838427947598253]
[]
[{"$nulls":11},"Measured compounds HI by X95",5.37045534887238]
[{"$nulls":11},"Without formaldehyde by X95",5.189819101516565,4.90597630675674]
[{"$nulls":11},"cancer by GM",1.0028400202020202,"Resp. ratio",0.5626632995650599]
[{"$nulls":11},"cancer by X95",4.697387091728056,"Resp. ratio",0.4932596767576676]